# Azurewave Release 2012/06/07
# NH665 bgn+BT+FM       Win8  TF810C
manfid=0x2d0
prodid=0x0552
vendid=0x14e4
devid=0x4361
boardtype=0x0547
boardrev=0x11
# this design has 2.4GHz SP3T switch
boardflags=0x00081200
nocrc=1
xtalfreq=37400
boardnum=22
macaddr=00:11:22:33:44:55
#nvram_override=1
cckdigfilttype=20            #20~26
ag0=255
aa2g=3
ccode=ALL
#pa0itssit=0x20
#pa0b0=0x1203
#pa0b1=0xfd99
#pa0b2=0xff29
rssismf2g=0xa
rssismc2g=0x3
rssisav2g=0x7
maxp2ga0=0x46
sromrev=3
#il0macaddr=00:11:22:33:44:55
wl0id=0x431b
cckPwrOffset=5
ofdmdigfilttype2g=4
ofdm2gpo=0x44444444
mcs2gpo0=0x6666
mcs2gpo1=0x6666
swctrlmap_2g=0x44844484,0x4a8a4282,0x42824282,0x818a82,0x1ff
swctrlmap_5g=0
#noise_cal_ref_2g=53
rfreg033=0x19
rfreg033_cck=0x1f
dacrate2g=160
txalpfbyp2g=1
bphyscale=17
cckPwrIdxCorr=-15
pacalidx2g=40
##pacalath2g=180
##pacalidx2g1=65
noise_cal_enable_2g=1
txgaintbl=1
#triso2g=9
sd_gpout=0
sd_gpval=1
sd_gpdc=0

#for BT-coexistence
btc_params80=0
